# Fit Accumulated Damage Models and Estimate Reliability using ABC

## Documentation for package ‘abcADM’ version 1.0

- DESCRIPTION file.

## Help Pages

abcMCMC | ABC-MCMC for load duration experiment data
catConstants | Display the current constants
constLoad_4500_1Y | Example data with tau_c = 4500 and t_c = 1Y (8760 hours)
default_param | Default theta
print_LoadProfile | Print the load profile parameters
sample_load_profile | Residential load profile
set_LoadProfile | Set load profile
set_returnPeriod | Set end time of reliability assessment
set_simuSampleSize | Set the number of simulated samples
set_timeStep | Set time step
simu_failTime | Simulate samples of failure time using parameters theta
solveCanADM | Simulate the time-to-failures given theta (posterior samples) under load profile